Push the pushbutton to take data.

Press the screen dots to change modes:

Yellow: Record one data point

Blue: Record continuously, or pause

Green: Record a group of points

Red LED flashes when data is recorded.

Red LED full on indicates missing SD card.